**LED FLASH/Flash Ultra Dance Floor Tips:**

* Face all panels the same way.
* No more than 10 panels connected to same power electrical outlet (MAX 15)
* Leave a couple inches apart, to ensure when moving together, cords don’t become unplugged.
* When disconnecting, always put dmx cables on top first to ensure they’re not connected.
* Master is the panel with no red dot; red dot means slave
* Power consumption 80watts per floor

**Troubleshooting:**

If not responding to signal, try disconnecting, reconnecting DMX from beginning. Should eventually work.

**LED FLASH/Flash Ultra DMX**

|  |  |  |
| --- | --- | --- |
| 1 | Main Program | Full to allow for solid colours203-208 – sound active |
| 2 | Main Program Speed/ Full Colour Solid  | Low – quick clockwise/lightHigh – quick counter clock/Dark |
| 3 | Ultra – Strip Size |  |
| 4 | Ultra – Strip colour |  |
| 5 | ? |  |
| 6 | Ultra - Speed |  |
| 7 | Strobe | Only strip & Program |
| 8 | BLUE SOLID | ENSURE 1+2 Maxed |
| 9 | GREEN SOLID | ENSURE 1+2 Maxed |
| 10 | RED SOLID | ENSURE 1+2 Maxed |

|  |  |
| --- | --- |
| Blue |  |
| Green |  |
| Red |  |
| Purple | R+B |
| White | R+G+B |
| Turquoise | G+B |
| Yellow | R+G |
| Orange | Green 30% + Red 100% |